{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":81,"n_cols":7,"rows_kept":81,"merged":[[0,0,0,6],[2,0,8,0],[9,0,18,0],[19,0,26,0],[27,0,30,0],[31,0,34,0],[35,0,38,0],[39,0,41,0],[42,0,43,0],[44,0,49,0],[50,0,51,0],[52,0,58,0],[59,0,60,0],[59,1,60,1],[59,2,60,2],[59,6,60,6],[61,2,61,6],[62,2,62,6],[63,2,63,6],[64,0,65,0],[64,6,65,6],[68,0,68,6],[69,0,73,0],[74,0,74,6],[75,0,80,0]],"flags":["formulas_cached_only"]}
["英国Alphasense公司电化学气体传感器"]
["气体种类","产品型号","简单描述","测量范围ppm","分辨率（ppm）","抗过载（ppm）","备注"]
["氧气","O2-A1","φ20.0X16.8一年寿命",{"v":0.3,"d":"30%"},"非线性0.6%",null,"200~240μA @ 20.9% O2"]
[null,"O2-A2","φ20.0X16.8两年寿命",{"v":0.3,"d":"30%"},"非线性0.6%",null,"80~120μA @ 20.9% O2"]
[null,"O2-A3","φ20.0X16.8三年寿命",{"v":0.3,"d":"30%"},"非线性0.6%",null,"65~85μA @ 20.9% O2"]
[null,"O2-C2","φ20.0X23.0两年寿命抗烟气",{"v":0.3,"d":"30%"},"非线性0.6%",null,"80~120μA @ 20.9% O2"]
[null,"O2-C3","φ20.0X23.0两年寿命抗烟气",{"v":0.3,"d":"30%"},"非线性0.6%",null,"65~85μA @ 20.9% O2"]
[null,"O2-G1","φ20.0X10.2一年寿命小尺寸",{"v":0.3,"d":"30%"},"非线性0.6%",null,"65~85μA @ 20.9% O2"]
[null,"O2-G2","φ20.0X10.2两年寿命小尺寸",{"v":0.3,"d":"30%"},"非线性0.6%",null,"20~42μA @ 20.9% O2"]
["一氧化碳","CO-AE","φ20.0X16.5大量程",10000,5,100000,"12~20nA/ppm"]
[null,"CO-AF","φ20.0X16.5有过滤",5000,0.5,10000,"55~90nA/ppm"]
[null,"CO-AX","φ20.0X16.5抗氢",2000,0.5,4000,"55~90nA/ppm"]
[null,"CO-BF","φ32.0X16.5有过滤",5000,0.5,10000,"80~120nA/ppm"]
[null,"CO-BX","φ32.0X16.5抗氢",2000,0.5,5000,"70~120nA/ppm"]
[null,"CO-CE","φ20.0X23.0大量程抗烟气",10000,5,100000,"12~20nA/ppm"]
[null,"CO-CF","φ20.0X23.0有过滤抗烟气",5000,0.5,10000,"55~90nA/ppm"]
[null,"CO-CX","φ20.0X23抗氢抗烟气",2000,0.5,4000,"55~90nA/ppm"]
[null,"CO-DF","φ14.5X8.4迷你尺寸有过滤",1000,1.5,2000,"30-48nA/ppm"]
[null,"CO-D4","φ14.5X8.4迷你尺寸4PIN",1000,1.5,2000,"30-48nA/ppm"]
["硫化氢","H2S-A1","φ20.0X16.5",100,0.05,500,"550-875nA/ppm"]
[null,"H2S-AH","φ20.0X16.5大电流",50,0.03,250,"950-1400nA/ppm"]
[null,"H2S-AE","φ20.0X16.5大量程",2000,0.5,10000,"70-100nA/ppm"]
[null,"H2S-B1","φ32.0X16.5",200,0.05,500,"300-440nA/ppm"]
[null,"H2S-BH","φ32.0X16.5大电流",50,0.02,200,"1500-2000nA/ppm"]
[null,"H2S-BE","φ32.0X16.5大量程",2000,0.5,10000,"80-115nA/ppm"]
[null,"H2S-D1","φ14.5X8.4迷你尺寸",100,0.2,400,"110-160nA/ppm"]
[null,"H2S-D4","φ14.5X8.4迷你尺寸4pin",100,0.2,400,"110-160nA/ppm"]
["二氧化硫","SO2-AE","φ20.0X16.5大量程",2000,1.5,10000,"55-80nA/ppm"]
[null,"SO2-AF","φ20.0X16.5两年寿命",50,0.1,75,"450-750nA/ppm"]
[null,"SO2-BF","φ32.0X16.5两年寿命",100,0.1,500,"300-440nA/ppm"]
[null,"SO2-D4","φ14.5X8.4迷你尺寸4PIN",20,0.2,50,"180-300nA/ppm"]
["一氧化氮","NO-A1","φ20.0X16.5两年寿命",250,0.2,800,"320-480nA/ppm"]
[null,"NO-AE","φ20.0X16.5大量程",5000,1,10000,"60-100nA/ppm"]
[null,"NO-B1","φ32.0X16.5两年寿命",250,0.15,1200,"400-660nA/ppm"]
[null,"NO-D4","φ14.5X8.4迷你尺寸4PIN",100,0.2,200,"500-750nA/ppm"]
["二氧化氮","NO2-A1","φ20.0X16.5两年寿命",20,0.02,100,"-400 ~ -750nA/ppm"]
[null,"NO2-AE","φ20.0X16.5大量程",200,0.1,1000,"-400 ~ -750nA/ppm"]
[null,"NO2-B1","φ32.0X16.5两年寿命",20,0.02,100,"-600 ~ -1100nA/ppm"]
[null,"NO2-D4","φ14.5X8.4迷你尺寸4PIN",20,0.1,60,"-250 ~ -450nA/ppm"]
["氯气","CL2-A1","φ20.0X16.5两年寿命",20,0.02,50,"-350 ~ -650nA/ppm"]
[null,"CL2-B1","φ32.0X16.5两年寿命",20,0.02,60,"-600 ~ -950nA/ppm"]
[null,"CL2-D4","φ14.5X8.4迷你尺寸4PIN",20,0.1,60,"-200 ~ -375nA/ppm"]
["催化燃烧式","CH-A3","φ20.0X16.5","0-100LEL","灵敏度21～24mV / % ",null,"3V供电，抗中毒，防爆"]
[null,"CH-D3","φ14.5X8.4小尺寸","0-100LEL","13～18.5mV / % ",null,"3V供电，抗中毒，防爆"]
["二氧化碳","CO2-D1","φ14.5X8固态电解质原理","0.2～95%","6-10mv/ (0.55-5%CO2)",null,"2年寿命，2电极mV输出，低成本"]
[null,"CO2-D1调节板","35*55mm","0.2～95%","mV输出",null,"3V纽扣电池供电，30uA低功耗，2线制mV输出"]
[null,"IRC-A1","φ20.0X16.5 NDIR 红外原理","0-100 % vol","最高分辨率1ppm",{"v":1,"d":"100%"},"双波红外，高精度1％FS，长寿命"]
[null,"IRC-TM变送板","35*70mm","0~5000PPM,5%,20%,100%VOL","±50PPM from 5000ppm",{"v":1,"d":"100%"},"7～40V供电，4～20mA和USB输出，小尺寸"]
[null,"Cirius 2","φ20.0X16.5 NDIR 红外原理","0～5000ppm，0～5%VOL","<2%FS",{"v":0.05,"d":"5%"},"全金属结构，双波红外，有主动，参考和温度输出。"]
[null,"Cirius 3","φ20.0X16.5 NDIR 红外原理","0～5%VOL & 0～100%VOL","<2%FS",{"v":1,"d":"100%"},"全金属结构，双波红外，有主动，参考和温度输出。"]
["环氧乙烷","ETO-A1","φ20.0X16.5两年寿命",100,0.1,200,"1600-2000nA/ppm"]
[null,"ETO-B1","φ32.0X16.5两年寿命",100,0.1,500,"1500-2500nA/ppm"]
["特殊毒气","PH3-A1","φ20.0X16.5两年寿命",10,0.03,50,"1000-1500nA/ppm"]
[null,"PH3-B1","φ32.0X16.5两年寿命",10,0.05,150,"800-1100nA/ppm"]
[null,"PH3-BE","φ32.0X16.5两年寿命大量程",2000,2,5000,"15-25nA/ppm"]
[null,"HCL-A1","φ20.0X16.5一年寿命",25,0.4,50,"120-160nA/ppm"]
[null,"HCN-A1","φ20.0X16.5两年寿命",100,0.05,150,"60-80nA/ppm"]
[null,"HCN-B1","φ32.0X16.5两年寿命",100,0.05,200,"80-120nA/ppm"]
[null,"HCN-D4","φ14.5X8.4迷你尺寸4PIN",50,0.3,250,"25-40nA/ppm"]
["CO/H2S两用传感器","D2","φ14.5X8.4可测量CO/H2S两种气体","1000（CO）",1,5000,"新产品\n有4横针脚"]
[{"$nulls":3},"100（H2S）",0.25,400]
["氧气变送器","A系列","O2-A2 的变送器，4-20mA输出"]
["有毒气体变送器","B系列","7．5V—35VDC宽电压供电，超稳定，4-20mA输出，可调节零点和满量程。  "]
["数字变送器","兼容A系列和B系列","10V—30VDC宽电压供电，4-20mA输出，兼容A系列和B系列，温度补偿，超稳定，可与PC通讯修改量程和偏置电压等。"]
["光离子检测器PID","PID-AH","φ20.0X16.5 ppb级","5ppb~50ppm","灵敏度>20mV/ ppm异丁烯",50,"测量大部分可挥发有机物，精确到ppb级"]
[null,"PID-A1","φ20.0X16.5 ppm级大量程","100ppb~300ppm","灵敏度>1mV/ ppm异丁烯",6000]
["红外CH4","Cirius 1","φ20.0X16.5 NDIR 红外原理","0～100%LEL HC,0～100%VOL CH4","<2%FS","100%VOL","全金属结构，双波红外，有主动，参考和温度输出。"]
["红外传感器变送板","Cirius X","配合Cirius传感器使用","0～100%LEL HC/CO2,0～100%VOL CH4/CO2","<2%FS","100%VOL","8～36V供电，4～20mA和RS232输出，可选LCD显示"]
["英国GSS公司红外CO2传感器"]
["红外CO2传感器","C20","40mm*25mm*23mmAl-In-Sb锑化铟铝，LED NDIR","0～5%、10%、20%、65%、100%","10ppm,100%量程为100ppm","100%VOL","英国GSS公司专利的CO2传感器\n快速响应<4S，低功耗100mW"]
[null,"C20EV",null,"视传感器而定","100ppm",null,"9V供电，2行LCD显示，RS232串口通讯"]
[null,"C20E","40mm*25mm*23mmAl-In-Sb锑化铟铝，LED NDIR","0～5%","10ppm","100%VOL","温度补偿范围0～40度，专为教育行业设计"]
[null,"C20B","40mm*25mm*23mmAl-In-Sb锑化铟铝，LED NDIR","0～65%","10ppm","100%VOL","温度补偿范围0～40度，大量程，专为垃圾填埋，农村沼气检测而设计"]
[null,"C100","Φ43mmAl-In-Sb锑化铟铝，LED NDIR","0～2%","10ppm","100%VOL","温度补偿范围-25～55度，专为HVAC,IAQ行业设计"]
["英国SST公司氧化锆氧传感器"]
["氧化锆氧传感器","O2S-FR-T3","迷你型氧传感器","0.1～100％VOL",100,"100%VOL","低成本，允许气体温度范围-100～250度"]
[null,"O2S-FR-T4","法兰型氧传感器","0.1～100％VOL",100,"100%VOL","法兰安装，允许气体温度范围-100～400度"]
[null,"O2S-T2\nO2S-FR-T2","棒型氧传感器","0.1～100％VOL",100,"100%VOL","允许气体温度范围-100～250度"]
[null,"O2S-FR-T2-18C","螺纹型氧传感器","0.1～100％VOL",100,"100%VOL","螺纹安装，允许气体温度范围-100～250度"]
[null,"O2I-FLEX","经济型氧变送板","0.1～25％ & 100％VOL",100,"100%VOL","低成本，功能全,24V供电，4～20mA，0～10V，RS232输出"]
[null,"OXY-FLEX","氧分析仪","0.1～25％ & 100％VOL",100,"100%VOL","24V供电，4～20mA，0～10V，RS232输出"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}